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PRODUCT SPECIFICATIONS

INTRODUCTION
AMETCO® MANUFACTURING CORPORATION

*****  Ametco® Manufacturing Corporation manufacturers several types of ornamental metal fencing, railing systems, and sun shades from galvanized steel, stainless steel and aluminum.  In addition, many basic construction materials are provided such as perforated metal and plastic panels, expanded metal panels, wire cloth, steel and aluminum bar gratings, safety gratings, stair treads, and ladder rungs.  These can be used for custom designed shade canopies, play structures, signs, equipment screens, stairs, platforms, tables, benches, trash receptacles, sculptures are other custom fabrications.

PRODUCT SPECIFICATIONS

The following product guide specification sections have been prepared to assist design professionals in incorporating Ametco® fencing and other products into a competitive bid construction project.


Section 05 53 10 - Steel Bar Gratings


Section 05 53 11 - Aluminum Bar Gratings


Section 05 53 12 - Safety Gratings


Section 05 73 10 - Open Grille Steel Railing System


Section 05 75 10 - Perforated Metal Panels


Section 05 75 11 - Expanded Metal 


Section 05 75 12 - Wire Cloth


Section 06 60 10 - Perforated Plastic Panels


Section 10 71 14 – Metal Sun Shades


Section 32 31 17 - Ornamental Welded Wire Fencing


Section 32 31 20 - Ornamental Steel Fencing


Section 32 31 21 - Aluminum Louver Fencing


Section 32 31 22 - Stainless Steel Louver Fencing

The above numbers and titles are based on classifications and numbering contained in MasterFormat - Master List of Numbers and Titles for the Construction Industry, 2004 Edition, published jointly by the Construction Specifications Institute (CSI) and Construction Specifications Canada (CSC).  MasterFormat is a uniform system for organizing specification sections and other information in construction project manuals.  This industry standard allows for the quick and easy retrieval of construction information.

SECTION ORGANIZATION
The Ametco® Industries product guide specification sections have been organized according to SectionFormat - A Recommended Format for Construction Specification Sections, 1997 Edition, published jointly by CSI and CCS.  SectionFormat provides a uniform approach to organizing specification text by placing information in three standard parts:


PART 1 - GENERAL
Describes administrative and procedural requirements.


PART 2 - PRODUCTS
Describes materials, products, and accessories to be incorporated into the construction project.


PART 3 - EXECUTION
Describes how the products will be installed at the construction site.

WRITING STYLE
The Ametco® product specifications have been written using the writing principles and techniques contained in the Project Resource Manual published by CSI.  The goal is to develop specifications that are clear, correct, complete, and concise.  Within the Ametco® guide specifications, the imperative mood has been used for instructions for providing, fabricating, and installing products.  It is understood that the specifications are addressed to the contractor who is legally responsible to the owner for constructing the project.  Hence, the imperative mood is used to indicate actions to be performed by the contractor.  Following is an example of a requirement in the indicative mood and as a more direct imperative instruction.


Indicative mood:



Contractor shall attach plastic caps to tubular steel posts.


Imperative mood:



Attach plastic caps to tubular steel posts.

STREAMLINING
Unnecessary words such as "the", "an", and "a" have been eliminated.  Use of "for", "of", and other prepositions has been minimized.  Streamlining has also been used to reduce verbiage in the guide specifications.  This technique places the subject first and hence provides key words for quick reference.  The words "shall be" are included by inference where a colon (:) is used.  For example,


Standard phrasing:
 



The steel tubing used for fabricating the ornamental steel fencing shall be steel shapes complying with the requirements of ASTM A500 for Grade B.


Streamline phrasing:



Steel tubing:  ASTM A500, Grade B.

REFERENCES

Throughout the product specifications, references are made to other specification sections that might be contained in the project manual.  These references are presented as examples and coordination reminders.  For each project, these references will need to be revised to reflect actual sections being used.  The referenced specification section numbers and titles have been derived from the CSI/CSC MasterFormat.  Samples of references to be verified are:


Submit in accordance with Section 01 33 00 - Submittal Procedures: . . .


Coordinate fence and gate installation with provision of gate operator specified in Section  32 31 30 - Gate Operator.

EDITING

The Ametco® guide specifications will need to be edited by the specifier for a specific project and to reflect the products, options, and applications being used.  The specifications are on CD in the front cover of the binder.  The guide sections have been written so that most editing can be accomplished by deleting unnecessary requirements and options.  Depending on project requirements, some additional information will need to be added by the specifier.  Options are indicated by  [   ].  Notes to assist the specifier in selecting options and editing the specification guides are printed in bold and indicated with  *****.  For final editing, all brackets and notes will need to be deleted from the guides.  For example:


*****  Include the following paragraph if hinged swinging gates are required.  *****

Type:  Hinged swinging [single] [double] gate.

METRIC EQUIVALENTS

Notes within the product specifications list U.S. Imperial dimensions followed by metric equivalents derived from System International Metric (SI) in parentheses.  Within the specification text, Imperial dimensions are presented first in brackets followed by SI metric equivalents also in brackets.  Depending of project requirements, either the Imperial or the SI metric equivalents will need to be deleted.  For example, 


*****  Spacing for 80 percent visual blocking is 2-1/16 inches (52 mm) and for 100 percent blocking is 1-13/16 inches (46 mm).


Louver bars:  Extruded aluminum louver bars, [1-31/32 inches] [50 mm] wide, spaced at [[1-13/16] [2-1/16] inches] [[46] [52] mm].


COMMENTS

These product guide specifications have been developed to assist the design professional in incorporating Ametco® Manufacturing Corporation ornamental metal railing fences and railings into a construction project.  Hopefully, this guide will reduce the time and effort required to prepare a project specification.  Your questions, comments, suggestions, and additional information requests will be appreciated and useful in preparing future revisions.  Please respond to Ametco® Manufacturing Corporation by mail, telephone, fax, or E-mail.


AMETCO® MANUFACTURING CORPORATION


P.O. Box 1210


Willoughby, Ohio 44096


Telephone:

800-362-1360


Fax:


440-951-2542


E-mail:

www.Ametco®.com






